














v.LOGiC Intelligent Solution
Interface


V6-MIB

Compatible with various MIB systems 
in Audi, Porsche, Skoda and VW vehicles



















Product features


· Picture-in-picture mode combining after-market rear-view and front camera picture(s) with factory parking sensor graphics
· [bookmark: _Hlk516585789]Interactive lane lines with calibration function
· Simultaneous use of picture-in-picture factory parking sensor graphics and interactive lane lines
· Own on-screen display and setup
· Controls of AV sources (e.g. DVB-T Tuner, ...) by MIB system
· Rear-view camera input
· Automatic switching to rear-view camera input on engagement of reverse gear from all operation modes
· Front camera input
· Side camera inputs
· Side- or front camera activation via blinker signal
· Manual switching to cameras
· 2 trigger outputs (+12V max. 1A), separately adjustable switching events (CAN, ACC, camera, reverse gear)
· Compatible with all factory video accessories
· USB update-port for software-updates by consumer
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Legal Information

By law, watching moving pictures while driving is prohibited, the driver must not be distracted.  We do not accept any liability for material damage or personal injury resulting, directly or indirectly, from installation or operation of this product.  This product should only be used while standing or to display fixed menus or rear-view-camera video when the vehicle is moving, for example the MP3 menu for DVD upgrades.

Changes/updates of the vehicle’s software can cause malfunctions of the interface.   We offer free software-updates for our interfaces for one year after purchase.  To receive a free update, the interface must be sent in at own cost.  Labor cost for and other expenses involved with the software-updates will not be refunded. 


1. Prior to installation

[bookmark: _Toc244342526]Read the manual prior to installation. Technical knowledge is necessary for installation. The place of installation must be free of moisture and away from heat sources.


1.1. Delivery contents 

Take down the SW-version and HW-version of the interface boxes, and store this manual for support purposes.


LVDS cable
CAB-HSD-MG060-OZ

[image: Y:\aaa Produkte\Artikel\V3-CIC-E\Bild1_V3-CIC-E.png]Interface-box
V6C-M655
HW_____  SW_____





V4C-VIDEO harness





V6C-MIB01 harness


LVDS cable
CAB-HSD-FF150





[bookmark: _Hlk516587084]
1.2. [bookmark: _Toc244342527][bookmark: _Hlk516587005]Check compatibility of vehicle and accessories


Requirements



































	Brand
	Compatible vehicles
	Compatible systems

	Audi
	A3 (8V) from 05/2012-, A4 (8W) from 08/2015-,  Q7 (4M) ab 03/2015-
	MMI Navigation Plus with MMI touch 7"or 8.3" - MIB/MIB II main-unit

	Porsche
	Cayenne, Boxster, 911, Cayman
	PCM 4.0

	Skoda
	Octavia 2017-
	MIB - Amundsen 8”

	VW
	Golf7 MY 2015-, Golf7 Sportsvan MJ 2015-, Passat (B8) MY 2015-,
T-Roc MY 2017-
	MIB/MIB2 - Discovery Pro 8” and Composition Media - 6.5” monitor.




[bookmark: _Hlk516587132][bookmark: _Toc247086324]






1.3. Setting the dip switches of the interface-box V6C-M655

Dip 1 on the back of the interface-box V6C-M655 are used to set the monitor type. The default setting is:

	Vehicle
	[bookmark: _Hlk515956452]Monitor
	Dip 1
	Dip 2
	Dip 3

	[bookmark: _Hlk515956840]Audi A3 (8V), Audi A4 (8W) VW Crafter
	7“
	[bookmark: _Hlk515957173]ON
	[bookmark: _Hlk515957269]OFF
	OFF

	Audi A4 (8W)
	8,3“
	ON
	ON
	ON

	Audi Q7 (4M)
	8,3“
	[bookmark: _Hlk515957282]ON
	[bookmark: _Hlk515957302]OFF
	ON

	[bookmark: _Hlk515957107][bookmark: _Hlk515957060][bookmark: _Hlk520113416]Porsche Cayenne, Boxster, 911, Cayman
	7“
	ON
	ON
	OFF

	Skoda Octavia 3, MAN TGE
	8“
	OFF
	OFF
	ON

	VW Golf 7, Sportsvan
	6,5“
	OFF
	[bookmark: _Hlk515957313]ON
	OFF

	[bookmark: _Hlk517100531]VW Passat (B8)
	6,5“
	OFF
	ON
	ON

	VW Passat (B8), T-Roc
	8“
	ON
	ON
	OFF



After each change of the dip switch settings you have to execute a power reset of the interface-box!


1.4. LED‘s of the interface-box V6C-M655


[image: ]

























2. Connection scheme

[image: ]

3. Installation

Switch off ignition and disconnect the vehicle’s battery! The interface needs a permanent 12V source. If according to factory rules disconnecting the battery is to be avoided, it is usually sufficient to put the vehicle is sleep-mode.  In case the sleep-mode does not show success, disconnect the battery with a resistor lead.
[bookmark: _Toc244342535]If power source is not taken directly from the battery, the connection has to be checked for being start-up proven and permanent.
Prior to wire and device installation we suggest to connect and test correct function of all after-market and factory infotainment equipment!

The interface is installed on the backside of the head unit.

3.1. Connecting interface box and harnesses
[image: ]






























1

Disconnect Quadlock connector from the head unit and remove the 12pin connector 
from chamber "E".
2

[bookmark: _Hlk516059969]Plug in the original vehicle Quadlock 12Pin connector to the 12pin socket of the 
V6C-MIB01 harness.
3

Plug in the 12 pin connector of the V6C-MIB01 harness to chamber "E" of the vehicle 
[bookmark: _Hlk516059948]Quadlock connector.
4

[bookmark: _Hlk516060022]Connect red wire with +12V (Quadlock connector pin 18, chamber D) and black wire 
with ground (Quadlock connector pin 17, chamber D).
5

[bookmark: OLE_LINK17][bookmark: OLE_LINK18][bookmark: OLE_LINK13][bookmark: OLE_LINK14][bookmark: OLE_LINK11][bookmark: OLE_LINK12]Plug in the 18 pin AMP connector of the V6C-MIB01 harness to 18pin socket of the 
V6C-M655 interface.
6

Plug in the 14pin connector of the V4C-VIDEO harness to 14pin socket of the 
V6C-M655 interface and connect back the vehicle Quadlock to the head unit.


Connection assignment:
[image: CAS_FTP:CAS_FTP_SERVER:KFZ Daten:Audi:Radios:Audi_VW_Quadlock_2G.jpg]
	Cable colour
	Assignment

	●	Red
	+12V permanent - pin 18

	[bookmark: _Hlk516059844]●	Brown
	Ground - Pin 17

	[bookmark: _Hlk516059860]●●	Orange/Violett
	CAN HIGH - Pin 6

	●●	Orange/Brown
	CAN LOW - Pin 12





Quadlock





















3.2. [image: ]LVDS connection

















1

Connect the female 4pin HSD LVDS connector of the LVDS cable CAB-HSD-FF150
to the male 4pin HSD LVDS connector (LVDS IN) on the rear of the interface-box 
V6C-M655.
2

[bookmark: _Hlk531339500]Remove the gray / green(Porsche PCM4.0 only) or pink (MIB system specific) female 
4pin HSD LVDS connector of the vehicle harness at the back of the head unit and 
connect it to the male 4pin HSD LVDS of the CAB-HSD-MG060-OZ LVDS cable.
3

Connect the female 4pin HSD LVDS connector of the LVDS cable CAB-HSD-MG060-OZ
to the male 4pin HSD LVDS connector (LVDS OUT) on the rear of the interface box 
V6C-M655.
4

Connect the female 4pin HSD LVDS connector of the LVDS cable CAB-HSD-FF150
to the gray/green(Porsche PCM4.0 only)/pink male 4pin HSD LVDS connector on the 
rear of the head unit.














3.2.1. [bookmark: OLE_LINK69][bookmark: OLE_LINK70]After-market front camera
[image: ]
3.2.1.1. Connection to the after-market front camera





















1

Connect the video RCA of the after-market front camera to the female RCA connector “AV-1” of the V4C-VIDEO harness.
[image: ]2

The pink wire (12V OUTPUT 1) of harness V6C-MIB01 can be used for +12V electric power supply (max. 1A) of the after-market front camera. Configure in the OSD-menu “Option 1”, menu item “Power Out 1” the setting “CAM” (see also chapter “Configurable switching outputs”). 

















3.2.1.2. Settings for connecting an after-market front camera

[image: ][image: ][image: ]You have to configure some settings in the OSD-menus Inputs, Option 1 and Option 2 if you want to connect an after-market front camera (Operation of the OSD: see chapter “OSD-Operation”).

	OSD-menu
	Menu item
	Setting
	Explication

	Input
	
FVC
	OFF
	Front camera deactivated

	
	
	ON
	Switches to front camera if parking process is enabled and reverse gear is released

	



Option 1
	Park Logic
	Intelligent
	For vehicles with front-PDC. Enabled while parking process and up to 20 km/h

	
	
	RGearOnly
	Enabled while parking process
(not suitable for front camera operation)

	
	
	RGearSpeed
	Enabled while parking process and up to 
e.g. 10km (speed adjustable)

	
	
	RGearTime
	Enabled while parking process and up to 
20 second

	Option 2
	R/F Cam Till
	XX
	Speed setting for deactivating of the camera image

	Option 2
	PDC Graphic
	OFF
	[bookmark: _Hlk516650750]OEM PDC display of the vehicle deactivated

	
	
	Horizontal
	[bookmark: _Hlk531339138]Vehicles with horizontal OEM PDC display

	[bookmark: _Hlk531339232]
	
	Hor. Dark
	Vehicles with horizontal OEM PDC display – 
alternative presentation

	
	
	Vertical
	Vehicles with vertical OEM PDC display



[bookmark: OLE_LINK37][bookmark: OLE_LINK38][bookmark: OLE_LINK35][bookmark: OLE_LINK36]Note: You can deactivate the camera image by long pressing (2 sec.) the rotation knob. 
[bookmark: OLE_LINK109][bookmark: OLE_LINK110]

3.2.2. [bookmark: OLE_LINK3][bookmark: OLE_LINK4][bookmark: OLE_LINK1][bookmark: OLE_LINK2][bookmark: OLE_LINK41][bookmark: OLE_LINK42]After-market wide view front camera
[bookmark: OLE_LINK39][bookmark: OLE_LINK40][image: ]
3.2.2.1. Connection to the after-market wide view front camera





















1

Connect the video RCA of the after-market wide view front camera to the female RCA connector “AV-1” of the V4C-VIDEO harness.
[image: ]2

The pink wire (12V OUTPUT 1) of harness V6C-MIB01 can be used for +12V electric power supply (max. 1A) of the after-market front camera. Configure in the OSD-menu “Option 1”, menu item “Power Out 1” the setting “CAM” (see also chapter “Configurable switching outputs”). 




3

Exception: Connect the white/black wire of harness V6C-MIB01 to the right and left analogue blinker signals (triggered +12V blinker power) and make the menu setting - Option 2 / Cam Trigger - „Analogue“, if the system doesn’t switch to the aftermarket wide view front camera automatically after the described OSD-setup (Option 2 / Cam Trigger - „CAN“, see next chapter). 







3.2.2.2. Settings for connecting an after-market wide view front camera

[bookmark: OLE_LINK55][bookmark: OLE_LINK56]For the use of a wide view front camera, the interface offers not only manual activation, but also activation via the blinker function. Note: via CAN bus blinker signal detection (menu: Option 2 / Cam Trigger - "CAN“), the activation does not take place in "blinker comfort mode" (brief touch of the blinker lever).
[image: ]You have to configure some settings in the OSD-menus Inputs, Option 1 and Option 2 if you want to connect an after-market front camera (Operation of the OSD: see chapter “OSD-Operation”).
[image: ][image: ]

	OSD-menu
	Menu item
	Setting
	Explication

	Input
	
FVC
	OFF
	Front camera deactivated

	
	
	ON
	Switches to front camera if parking process is enabled and reverse gear is released

	



Option 1
	Park Logic
	Intelligent
	[bookmark: OLE_LINK64][bookmark: OLE_LINK65]For vehicles with front-PDC. Enabled while parking process and up to 20 km/h

	
	
	RGearOnly
	Enabled while parking process
(not suitable for front camera operation)

	
	
	RGearSpeed
	Enabled while parking process and up to 
e.g. 10km (speed adjustable)

	
	
	RGearTime
	Enabled while parking process and up to 
20 second

	Option 2
	R/F Cam Till
	XX
	Speed setting for deactivating of the camera image

	Option 2
	F/S Cam From
	XX
	[bookmark: OLE_LINK107][bookmark: OLE_LINK108]Speed range setting for front- and side cameras (minimum)

	Option 2
	F/S Cam Till
	XX
	Speed range setting for front- and side cameras (maximum)

	Option 2
	Blinker Mode
	Front Cam
	Activation of the front camera image when the blinker is activated

	[bookmark: _Hlk516218989]Option 2
	Cam Trigger
	CAN
	[bookmark: OLE_LINK45][bookmark: OLE_LINK46][bookmark: OLE_LINK15]Rear gear and blinker signal detection over CAN Bus

	
	
	[bookmark: OLE_LINK24][bookmark: OLE_LINK25]Analogue
	Rear gear and blinker signal detection over analogue +12V signals



Notes: You can deactivate the camera image by long pressing (2 sec.) the rotation knob. 
The camera activation via the blinker mode is only available for front camera or for the side view cameras. A parallel use of this function for all cameras is not possible.

[bookmark: OLE_LINK73][bookmark: OLE_LINK74]
3.2.3. After-market side view cameras
[image: ]
3.2.3.1. Connection of the after-market side view cameras





















1

[bookmark: OLE_LINK111][bookmark: OLE_LINK112]Connect the video RCA of the right side view camera to the female RCA connector “AV-2” and the video RCA of the left side view camera to the female RCA connector “AV-3”of the V4C-VIDEO harness.
[image: ]2

[bookmark: _Hlk520882000]The pink wire (12V OUTPUT 1) of harness V6C-MIB01 can be used for +12V electric power supply (max. 1A) of the after-market side cameras. Configure in the OSD-menu “Option 1”, menu item “Power Out 1” the setting “CAM” (see also chapter “Configurable switching outputs”). 




3

[bookmark: OLE_LINK117][bookmark: OLE_LINK118][bookmark: OLE_LINK115][bookmark: OLE_LINK116]Exception: Connect the yellow/red wire to the right analogue blinker signal and the yellow/green wire to the left analogue blinker signal of harness V6C-MIB01 (triggered +12V blinker power) and make the menu setting - Option 2 / Cam Trigger - „Analogue“, if the system doesn’t switch to the aftermarket side view camera automatically after the described OSD-setup (Option 2 / Cam Trigger - „CAN“, see next chapter). 


‘


3.2.3.2. Settings for connecting of after-market side view cameras

For the use of side view cameras, the interface offers not only manual activation, but also activation via the blinker function. Note: via CAN bus blinker signal detection (menu: Option 2 / Cam Trigger - "CAN“), the activation does not take place in "blinker comfort mode" (brief touch of the blinker lever).
[image: ]You have to configure some settings in the OSD-menus Inputs, Option 1 and Option 2 if you want to connect an after-market front camera (Operation of the OSD: see chapter “OSD-Operation”).
[image: ][image: ]

	OSD-menu
	Menu item
	Setting
	Explication

	Input
	Right VC
	ON
	[bookmark: _Hlk7016865]Right camera input activated

	
	Left VC
	ON
	Left camera input activated

	



Option 1
	Park Logic
	Intelligent
	For vehicles with front-PDC. Enabled while parking process and up to 20 km/h

	
	
	RGearOnly
	Enabled while parking process
(not suitable for front camera operation)

	
	
	RGearSpeed
	Enabled while parking process and up to 
e.g. 10km (speed adjustable)

	
	
	RGearTime
	Enabled while parking process and up to 
20 second

	Option 2
	R/F Cam Till
	XX
	Speed setting for deactivating of the camera image

	Option 2
	F/S Cam From
	XX
	Speed range setting for front- and side cameras (minimum)

	Option 2
	F/S Cam Till
	XX
	Speed range setting for front- and side cameras (maximum)

	Option 2
	Blinker Mode
	Side Cam
	Activation of the side view cameras image when the blinker is activated

	Option 2
	Cam Trigger
	CAN
	Rear gear and blinker signal detection over CAN Bus

	
	
	Analogue
	Rear gear and blinker signal detection over analogue +12V signals



Notes: You can deactivate the camera image by long pressing (2 sec.) the rotation knob. 
The camera activation via the blinker mode is only available for front camera or for the side view cameras. A parallel use of this function for all cameras is not possible.



3.2.4. After-market rear-view camera

3.2.4.1. Connection to the after-market rear-view camera
[image: ]





















1

Connect the video RCA of the after-market rear-view camera to the female RCA connector “R-CAM” of the V4C-VIDEO harness.
[image: ]2

The green wire (12V OUTPUT 2) of harness V6C-MIB01 can be used for +12V electric power supply (max. 1A) of the after-market rear-view camera. Configure in the OSD-menu “Option 1”, menu item “Power Out 2” the setting “CAM” (see also chapter “Configurable switching outputs”). 




3

Exception: Connect the white wire of harness V6C-MIB01 to analogue rear gear signal (+12V) and make the menu setting - Option 2 / Cam Trigger - „Analogue“, if the system doesn’t switch to the aftermarket rear-view camera automatically after the described OSD-setup (Option 2 / Cam Trigger - „CAN“, see next chapter). 







3.2.4.2. Settings for connecting an after-market rear-view camera

[image: ][image: ][image: ]You have to configure some settings in the OSD-menus Inputs, Option 1 and Option 2 if you want to connect an after-market rear-view camera (Operation of the OSD: see chapter “OSD-Operation”).

	OSD-menu
	Menu item
	Setting
	Explication

	Input
	
RVC
	OFF
	Rear-view camera deactivated

	
	
	ON
	Switches to rear-view camera if reverse gear is engaged or PDC is activate

	



Option 1
	Park Logic
	Intelligent
	For vehicles with PDC. Enabled while parking process and up to 20 km/h (not suitable for front camera operation for vehicles without front-PDC)

	
	
	RGearOnly
	Enabled while parking process
[bookmark: OLE_LINK47][bookmark: OLE_LINK48](not suitable for front camera operation)

	[bookmark: _Hlk516398366]
	
	RGearSpeed
	Enabled while parking process and up to 
e.g. 10km (speed adjustable)

	
	
	RGearTime
	Enabled while parking process and up to 
20 second

	[bookmark: _Hlk516239208]Option 1
	RVC Lines
	ON
	Interactive lane lines activated

	Option 2
	R/F Cam Till
	XX
	[bookmark: OLE_LINK68][bookmark: OLE_LINK71]Speed setting for deactivating of the camera image

	Option 2
	PDC Graphic
	OFF
	OEM PDC display of the vehicle deactivated

	
	
	Horizontal
	Vehicles with horizontal OEM PDC display

	
	
	Hor. Dark
	Vehicles with horizontal OEM PDC display – 
alternative presentation

	
	
	Vertical
	Vehicles with vertical OEM PDC display

	Option 2
	Cam Trigger
	CAN
	Rear gear and blinker signal detection over CAN Bus

	
	
	Analogue
	Rear gear and blinker signal detection over analogue +12V signals



Note: You can deactivate the camera image by long pressing (2 sec.) the rotation knob. 





3.2.4.3. Settings for OEM rear-view camera

	OSD-menu
	Menu item
	Setting
	Explication

	Input
	RVC
	OEM
	If a factory rear-view camera is existing!
The interface turns off, if reverse gear is enabled and it displays factory rear-view camera

	[bookmark: _Hlk516398224]Option 1
	Park Logic
	Intelligent
	For vehicles with front-PDC. Enabled while parking process and up to 20 km/h

	
	
	RGearSpeed
	Enabled while parking process and up to 
e.g. 10km (speed adjustable)

	
	
	RGearTime
	Enabled while parking process and up to 
20 second

	Option 2
	R/F Cam Till
	XX
	Speed setting for deactivating of the camera image


































3.2.5. AV source

[bookmark: _Hlk520881720]The AV-3 or AV-2 input can alternatively be used for AV source connection. In addition, the interface has the option of controlling the connected compatible AV source over the touchscreen / control knob.

3.2.5.1. [image: ]AV source video connection























1

Connect video RCA of AV source to female RCA connector "AV-3" or "AV-2" of the video harness V4C-VIDEO. 
2

[image: ] The pink wire (12V OUTPUT 1) of harness V6C-MIB01 can be used for +12V electric power supply (max. 1A) of the AV source. Configure in the OSD-menu “Option 1”, menu item “Power Out 1” the setting “AVS” or “ACC” (see also chapter “Configurable switching outputs”).
3

[bookmark: _Hlk520884792]Optional: Using the respective STA-xxx IR-control cable (available separately), interconnect the female 3pin AMP connector of harness V6C-MIB01 and the IR-port of the AV source.







3.2.5.2. [bookmark: _Hlk520795092][image: ]AV source audio connection










1

Connect the audio output of the AV source to the vehicle AUX input. 



3.2.5.3. Settings for connecting an AV source

You have to configure some settings in the OSD-menu Input if you want to connect an AV source (Operation of the OSD: see chapter “OSD-Operation”).

[image: ]







	OSD-menu
	Menu item
	Setting
	Explication

	[bookmark: _Hlk520814075]Input
	[bookmark: _Hlk520812583]Right VC/AV
	OFF
	No camera / AV source connected

	
	
	RCxx
	AV source connected to the AV-2 input

	
	Left VC/AV
	OFF
	No camera / AV source connected

	
	
	RCxx
	AV source connected to the AV-3 input



[bookmark: _Hlk520897899]Note: Select "RC01" if AV source control function via touchscreen / control knob is not used.













3.2.6. [image: ]Configurable trigger outputs

















[bookmark: _Hlk516488331]You can configure the both +12V trigger outputs separately. The pink wire is (12V OUTPUT 1) is Power Out 1  and the green wire is (12V OUTPUT 2) is Power Out 2.

Note: You can configure the both trigger outputs in the OSD-menu Option 1 separately (Operation of the OSD: see chapter “OSD-Operation”). 
[image: ]







	OSD-menu
	Menu item
	Setting
	Explication

	OPTION
	Power Out 1 (pink)

Power Out 2 (green)
	CAN
	+12V when the interface is on (red LED on)

	
	
	ACC
	+12V when ignition is on

	
	
	Cam
	[bookmark: _Hlk516500868]+12V when camera input is activated (manually or automatically)

	
	
	RGear
	+12V when reverse gear is engaged

	
	
	AVS
	[bookmark: _Hlk516501094]+12V when camera / video input was manually activated

	
	
	OFF
	Trigger output deactivated 




[bookmark: _Hlk516488833][bookmark: _Hlk516488813][bookmark: _Hlk520881542][bookmark: _Hlk520881557]Tip: We recommend for all camera modes the power out setting “Cam” and for AV source the power out setting “AVS” or “ACC”.





3.3. [bookmark: _Hlk516499957]Interactive lane lines
[image: ]
You have to configure some settings in the OSD menu 
Option 1 if you want to activate interactive lane lines 
(Operation of the OSD: see chapter “OSD-Operation”). 
[image: ]








	OSD-menu
	Menu item
	Setting
	Explication

	Option 1
	RVC Lines
	OFF
	Interactive lane lines deactivated

	
	
	ON
	Interactive lane lines activated

	
	Car Type
	AUDI_A3/AUDI_A4/
AUDI_Q7/PASSAT/GOLF_7/
[bookmark: _Hlk531339393]CAYENNE/911/Boxster/Cayman/Others
	
Vehicle type selection





3.3.1. [bookmark: _Hlk516501260][bookmark: _Hlk516494677]Interactive lane lines settings 

[image: ]The height and width of the interactive lane lines can be set in the
OSD menu. For this setting you must at first activate the rear-view
camera level and push then the „MENU“/„HOME“(Porsche) button 
[image: ]for 2sec. to activate the settings menu. With the rotation knob you 
can select the menu point "Line Height" to change the height of the 
interactive lane lines and with menu point "Line Width" the width 
of the lines. Over the menu point "Exit" you can leave this settings 
menu.

3.4. [image: ][image: ][image: ][image: ][image: ]Picture settings

The camera picture settings can be set in the OSD menu. 
For this setting you must at first activate the camera level 
and push then the „MENU“/„HOME“(Porsche) button for 
2sec. to activate the settings menu. With the rotation knob 
you can select and change the "Brightness", "Contrast", 
"Saturation", Hue" and "Sharpness" menu points.
Over the menu point "Exit" you can leave this settings menu. 





4. Operation

4.1. Main OSD On-screen display

You can change the basic configurations of the interface in the OSD (on screen display).
[image: ]









4.1.1. OSD – Operation

The OSD menu can be controlled via the following buttons:

4.1.1.1. [image: ]Audi OSD control


























4.1.1.2. [image: ]VW / Skoda OSD control




















4.1.1.3. [image: ]Porsche OSD control



























4.1.2. OSD – Additional setting options

The following settings in the OSD menus Option 1 and OSD can be configured over and above the described settings in this manual (Operation of the OSD: see chapter “OSD-Operation”):
[image: ][image: ][image: ]







	OSD-menu
	Menu item
	Setting
	Explication

	Osd
	POS. X
	0-xxx
	Horizontal position of the OSD

	
	POS. Y
	0-xxx
	Vertical position of the OSD 

	
	Size
	Small
	Small OSD menu windows

	
	
	Large
	Large OSD menu windows

	
	Osd TimeOut
	2-20
	Time setting for automatic OSD shutoff

	Info
	Version
	X.XX.XX
	Displays the current SW-version

	Option 1
	Factory Reset
	Resetting to factory settings








4.2. [image: ]Selecting the interface as current video source
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In the vehicle’s Media menu, activate AUX level (only necessary for AV source operation) and press long “MEDIA” button to choose the interface as current video source.

Short press ”MEDIA” button (or additionally on touchscreen the swipe gesture) switch the video sources (cameras/AV source). Each short press will switch to the next enabled input. If all inputs are enabled the order is:

[bookmark: _Hlk516575348]Rear CAM  Front CAM  Right Cam/AV  Left Cam/AV  …

Inputs which are not enabled are skipped.

The exiting of the video interface level is achieved by long press of “MEDIA” button or by short press of “RADIO/TUNER/NAV/MAP/TEL/PHONE/SOURCE/CAR” (MIB system specific) button.


4.3. Assigning device controls
[image: ]
You can assign the device controls in the OSD-menu Input (Operation of the OSD: see chapter “OSD-Operation”). Assign related IR-codes for Left VC/AV or Right VC/AV input as described in device control table (see appendix A).


Note: Select "RC01" if AV source control function via touchscreen / control knob is not used.


4.4. Controlling of the connected AV source

The picture shows which functions of the connected devices can be executed by touch screen / control knob. Once an AV-input is activated the touchscreen control knob action will execute the function described in the picture. The function description equals the remote control buttons of the device’s remote control. On the additional device the writing on the remote control buttons may vary (e.g. AV instead of Source).

4.4.1. Audi AV source control
[image: ]






















Note: A few functions could be different on some connected devices.




4.4.2. VW / Skoda AV source control
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Note: A few functions could be different on some connected devices.

4.4.3. [image: ]Porsche AV source control




















[bookmark: _Hlk520895298][bookmark: _Hlk520895649]

Note: A few functions could be different on some connected devices.

5. Specifications

Operation voltage			10.5 – 14.8V DC
Stand-by power drain            		1mA
[image: ]Operation power drain		190mA
Power consumption			2,6W
Temperature range			-20°C to +80°C
Weight	 (box only)			285g
Measurements (box only) B x H x T	141 x 30 x 105 mm

[image: ]
6. Connections (interface-box)
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